Build 3.9.0.0
Release Notes:
•	PSSCON-1319: Handled crashing when selecting "Cancel" when opening .dis file in Convergence.
•	PSSCON-1316: Signalmaster sync visibility for configuration that have configured.
•	PSSCON-1315: Check added for devices in Bootload before allowing users to update.
•	PSSCON-1314: Device Version comparison to Software firmware when user has no Internet.
•	PSSCON-1312: Handled crashing when switching between CANDiag and Diag too quickly.
•	PSSCON-1311: Add random seed to 200 config file to randomize checksum and force siren update.
•	PSSCON-1308: Removed "Remote Handheld" from description under FSDirect in interface splashscreen.
•	PSSCON-1307: Erased function added to Device toolbar options.
•	PSSCON-1306: Play All pattern option added for Dynaflare
•	PSSCON-1305: Add Cruise I-IV for Vision.
•	PSSCON-1304: Separate Lightbar Device Page models by family selection.
•	PSSCON-1303: Separate Lightbar models by family selection.
•	PSSCON-1302: Separate Amplifier models by family selection.
•	PSSCON-1291: Add PA300-200 Siren to the Convergence Network software.
•	PSSCON-1117: FSJoin 4 Channel Expansion Module.
Build 3.8.0.8
Release Notes:
•	PSSCON-1296: Fixed an issue where previous Discrete process tables were not being properly overwritten.
•	PSSCON-1294: Updated firmware images for all FSJoin devices to version (1.4.2.5).
•	PSSCON-1293: Released new firmware versions: Pathfinder – (3.2.0.27) PF400 / PF400Q – (1.0.0.33) PathWay – (1.1.0.21) HDMod – (1.0.0.41) Keypad – (3.1.0.21) Sync (1.3.0.2)
•	PSSCON-1292: Added 2026 Ford F59, 2024 Peterbilt 520, and 2023 Battle Motors LNT to the GUI.
•	PSSCON-1290: Removed Lightbar GPS from the Valor diagnostic screen.
•	PSSCON-1289: Devices will no longer be erased when below the flash remaining threshold.
•	PSSCON-1288: Resolved a programming issue where PF400 devices failed to retrieve directories correctly.
•	PSSCON-1287: Added Pop feature support for all colors on FSJoin Lightbars and DynaFlares.
•	PSSCON-1286: Corrected programming behavior when using multiple DynaFlares with different module counts to ensure proper head stretching.
•	PSSCON-1285: Fixed an issue where dragging grouped relays while scrolling limited selection.
•	PSSCON-1284: Updated Discrete GUI label to include “+ BROWN” in “RED + YELLOW (Mode 2)”.
•	PSSCON-1283: Added numbering to relay wiring report pages.
•	PSSCON-1281: Improved ProcessLoader stability when importing CSV files containing extra spaces.
•	PSSCON-1280: Added Signalmaster support for DynaFlares.
•	PSSCON-1278: Added fuse cutoff support in diagnostics based on configured current limits.
•	PSSCON-1277: Added support for Speakers 3 and 4 in the Tone Wizard for PF400/PF400Q devices.
•	PSSCON-1276: Added 2026 Ford vehicle lineup to the GUI.
•	PSSCON-1275: Fixed FS Fade Pulse clearing within relay grouping.
•	PSSCON-1273: Increased the size of the amplifier bootload recovery window for better usability.
•	PSSCON-1272: Fixed BarcodeProcessLoader AlgtMax issue when a head was set to D (White/Green) on the PE board.
•	PSSCON-1270: Added the ability to assign custom names to FSJoin relay devices.
•	PSSCON-1268: Corrected AlgtMax Puddlelight so it is no longer affected by legacy Flashing Takedown or Flash Patterns.
•	PSSCON-1267: Resolved an InvalidOperationException when loading configurations that support Color & State but were missing required data.
•	PSSCON-1266: Added a warning prompt when selecting a different amplifier model or keypad type.
•	PSSCON-1265: Added buttons 18–21 to support remote activation.
•	PSSCON-1264: Added support for 2025 Ford Low/Manual transmission range and 2025 Rizon E18L.
•	PSSCON-1263: Fixed a crash that occurred when deleting a DynaFlare while on the splash screen.
•	PSSCON-1260: Added Force Play timer option to CAN buttons.
•	PSSCON-1258: Updated the default FSJoin Relays tab layout to prioritize Relays and Grouped Relays over the Pattern Selector.
•	PSSCON-1257: Local Keypad now properly initializes rotary dial backlights on new devices.
•	PSSCON-1256: Tooltips now display correctly when hovering.
•	PSSCON-1255: DynaFlare updates no longer trigger unnecessary warning messages.
•	PSSCON-1195: Added support for cloud-based firmware updates.
Build 3.8.0.0
Release Notes:
•	PSSCON-1252: Create Discrete Lightbar Programming interface.
•	PSSCON-12249: Added 2025/2026 Isuzu/Freightliner vehicle data.
•	PSSCON-1244: Added support for dynamically assigning DynaFlare devices. 
•	PSSCON-1243: Introduced new support for relay grouping.
•	PSSCON-1235: Prevent the computer from entering sleep mode during firmware updates.
•	PSSCON-1232: Added support for up to 12 DynaFlares.
•	PSSCON-1231: Added proper support for “Pass” and “Driver Only” ILS modes.
•	PSSCON-1195: Implemented cloud-based firmware updates.
•	PSSCON-1237 :Updated controller firmware versions: HD_MOD: 1.0.0.40 Keypad: 3.1.0.18 Pathway: 1.1.0.19 PF200: 3.2.0.26 PF400/PF400Q: 1.0.0.31 SIM: 1.2.0.15
•	PSSCON-1228: Sync Module firmware update to version 1.3.0.0.
•	PSSCON-1236: Added automatic firmware assignment AlgtMax autodetect command.
•	PSSCON-1241: Fixed issue where the database-update popup blocked the close (X) button on the database notes window.
•	PSSCON-1238: The “Beep Reminder” option is now selectable only when “Beep Enable” is checked.
•	PSSCON-1233: Fixed “Cannot create new feature. Limit reached.” error popup on the Relay tab.
•	PSSCON-1219: Added 2024-2026 Chevy/Dodge/Jeep/GMC vehicle data.

Build 3.7.0.1
Release Notes:	
•	PSSCON-1228: Updated Sync Module to v1.3.0.0 to support GPS/ALS off/on. 
•	PSSCON-1227: Added ‘With GPS’ option for Allegiant Max lightbars. Added logic to turn off Sync Module GPS if Allegiant Max GPS is on.
•	PSSCON-1226: Added a custom message to inform users that only one DynaFlare device can be connected during updates.
•	PSSCON-1225: Fixed an issue where the keypad backlight level was not correctly restored on file load; it now loads the appropriate setting.
•	PSSCON-1224: Improved Bootloader Recovery Mode for enhanced stability and reliability.
•	PSSCON-1213: Fixed an issue where the application could crash when clicking the "+" button under Keypad LEDs in the Miscellaneous tab for 17-Button W/Rotary devices.
•	PSSCON-1212: Added support for Blink modes 1–4 on 17-Button W/Rotary and 13-Button keypads, enhancing LED feedback customization.
•	PSSCON-1208: Added checks for dependency removeable from absent CAN messages.
•	PSSCON-1207: Vehicle Database Release Notes added under Help toolbar. Release notes appear after updating Database.
•	PSSCON-1206: Fixed issue where Dyna Flare MID configuration was being reset when loading default configurations.
•	PSSCON-1205: Added support for Dyna Flare firmware version (1.4.1.5).
•	PSSCON-1203: Resolved bedlight activation issue that required deselecting and reselecting White color option.
•	PSSCON-1200: Fixed default head configuration for 53" and 61" Allegiant Max bedlights where some heads were incorrectly defaulting to Amber instead of White.
•	PSSCON-1189: Dyna Flare Wire Location displayed.
•	PSSCON-1183: Fixed application crash when DetectLed functionality was used without a NextGen Lightbar present in the configuration.

Build 3.7.0.0
Release Notes:
•	PSSCON-1179: New RLNT S2 Firmware (1.3.0.7).
•	PSSCON-1173: Clarified Save Workflow: When creating a new file from scratch, File → Save or Ctrl+S will now prompt you to use Save As first.
•	PSSCON-1167: New PF200 Default Configurations for (Local Keypad, Remote Keypad, Remote Handheld, 6 Button, Nine Button).
•	PSSCON-1164: 32 Channel Relay wiring report – Corrected input-to-relay correlation.
•	PSSCON-1162: PF400/PF400Q Relay wiring report bug fixed.
•	PSSCON-1161: Added default configurations for 13-button keypad.
•	PSSCON-1160: Sweep T13 – Added Title 13 and SAE compliance label.
•	PSSCON-1157: Current limit settings – Fixed issue with persistence for relay devices in popup.
•	 PSSCON-1153: PF200S17BRK Remote PA – Fixed default configuration issue.
•	PSSCON-1149: New Firmware images released – HD_MOD (1.0.0.36), Pathfinder (3.2.0.21), Keypad (3.1.0.13), PF400/PF400Q (1.0.0.26), Pathway (1.1.0.14), SIM (1.2.0.12), SYNC (1.2.1.0).
•	PSSCON-1089: New Cloud Support for Application updates and Can Data.
•	PSSCON-1010: New Allegiant Max tri-color lightbars (45", 53", 61", 70", 80").
•	PSSCON-904: New DynaFlare Lights.

Build 3.6.0.14
Release Notes:
•	PSSCON-1144: Added default configurations for 21 Button and 17 Button w/ Rotary for PF200, PF400, and PF400Q.
•	PSSCON-1143: Updated Left/Right Lamp signal for 2023 Chevy Silverado 1500, 2024 Chevy Silverado 1500/2500/3500 and 2025 Chevy Tahoe/Blazer EV. Added 2023 Chevy Silverado 2500/3500 CAN data.
•	PSSCON-1142: Added FSDirect Training Guide under Help dropdown menu.
•	PSSCON-1140: Logic to handle missing/replaced CAN data to remove dependencies from other inputs.
•	PSSCON-1138: Fixed buttons not showing an “Off” light on keypad.
•	PSSCON-1135: Updated OBDMOD16 Quick Start guide.
•	PSSCON-1134: Added CAN data for 2025 Ford Escape/Mustang/Maverick/Ranger/F450/F550/F650 and updated changes for 2024 Chevy Tahoe.
•	PSSCON-1132: Multiple Button Property fields now update on text field change instead of when the field loses focus.
•	PSSCON-1131: Changed message for Relays 17-18 on OBDMOD16 to reflect the lack of current sensing capabilities.
•	PSSCON-1130: Adjusted on/off delay for 24 Channel Module relays in Diagnostic mode.
•	PSSCON-1129: Added CAN data for 2024 Chevy Silverado 3500/Tahoe, Dodge Challenger/Charger/Ram 1500 SSV/Ram 2500, Ford Maverick/PIU/E-Transit, GMC Sierra 1500/Sierra 2500/Sierra 3500, International HV, Freightliner Custom FCCC MT55e/M2 Series, Toyota Tacoma, and 2025 Chevy Silverado 1500 and GMC Sierra 1500.
•	PSSCON-1126: Fixed 21” Allegiant front bedlight auto-detect
•	PSSCON-1124: New PF400/PF400Q Firmware Image Version (1.0.0.23).
•	PSSCON-1123: New Valor/Integrity Firmware Image Version (1.3.0.1).
•	PSSCON-1122: New Pathway Firmware Image Version (1.1.0.11).
•	PSSCON-1121: New Pathfinder Firmware Image Version (3.2.0.18).
•	PSSCON-1120: Fixed user-defined button names for Inputs 1–4 would display default labels until the input was manually selected after reloading the configuration.
•	PSSCON-1119: FSJoin Device Data Now Properly Removed from Configuration Upon Deletion.
•	PSSCON-1118: Removed Irrelevant References During OBDMOD16 Programming.
•	PSSCON-1116: Keypad Configuration Issues Resolved When Re-adding Devices.
•	PSSCON-1115: Corrected LegacyMode Pattern Indexing.
•	PSSCON-1114: SIM Inputs Now Fully Removed from Diagnostics When Associated Device is Deleted.
•	PSSCON-1113: Fixed incorrect conversion of HoldDuration values caused inputs to trigger immediately instead of respecting the specified delay.
•	PSSCON-1112: New HD Module Firmware Image Version (1.0.0.33).
•	PSSCON-1111: New 2025 Silverado 2500, 2023 - 2024 Silverado Sierra turn Signals, Brake Position, RPM, Throttle Position fixed and new Button Status Can Message.
•	PSSCON-1110: Tone Wizard no longer crashes GUI when options are Null.
•	PSSCON-1106: CAN Inputs now separated from Button Properties in the sidebar for improved clarity.
•	PSSCON-1104: Corrected modifier assignments for tone associations based on ToneID range.
•	PSSCON-1103: Fixed issue with EQ2B rotary backlighting not functioning.
•	PSSCON-1101: Resolved PID check behavior for Local/Remote PA on configuration load.
•	PSSCON-1100: Firmware updates added for Keypad Version (3.1.0.9), ALGT Version (1.3.0.2), HD Module Version (1.0.0.30), and SIM Version (1.2.0.9).
•	PSSCON-1099: Fixed diagnostics display for Feature State On/Off related to some inputs.
•	PSSCON-1097 : Custom Wiring Report now correctly updates relay names for OBDMOD16.
•	PSSCON-1096: Fixed crash when generating "Configuration Report" for relays with FSJoin fade patterns.
•	PSSCON-1095: Added CAN data for 2025 International HV.
•	PSSCON-1094: Added CAN data for 2025 Peterbilt.
•	PSSCON-1093: Sidebar properties now close correctly when switching configuration files.
•	PSSCON-1092: Prevented GUI failure when trying to add relays or siren functions with a full feature set.
•	PSSCON-1091: FSJoin relays now properly show active relays in the sidebar tree.
•	PSSCON-1090: Alarm dropbox now only appears for Local PA if it existed in the configuration prior to 3.6.0.3.
•	PSSCON-1088: Fixed incorrect language assignments on channels caused by inconsistent SirenChannelType mapping.
•	PSSCON-1087: Ensured only one valid 'Channel 3' entry per voice message configuration.
•	PSSCON-1086: Resolved crash in Configuration Viewer when using 32-channel BCM.
•	PSSCON-1085: Fixed issue where selected languages for voice messages were not being applied.
•	PSSCON-1084: Update Vehicle Database to 2025 FPIU Rear Hardwire.
•	PSSCON-1083: Fixed 32-Channel EXP module behavior after add/remove/add sequence in SplashScreen.
•	PSSCON-1082: MultiTap Toggle & Momentary MultiTap Duration now load and save correctly.
•	PSSCON-1081: Improved error messaging when programming the wrong device.
•	PSSCON-1080: Resolved intermittent programming failure for PF400Q devices with large file directories.
•	PSSCON-1079: Updated CAN database; added and fixed support for Doors (Any *) messages.
•	PSSCON-1078 : Added CAN data support for 2025 Ford F-150 and Transit.
•	PSSCON-1077: Fixed issue with MultiTap not being saved in the configuration.
•	PSSCON-1075: Added CAN data for 2024 Bronco and 2025 Bronco Sport.
•	PSSCON-1073: Addressed crash when loading .ptek files.
•	PSSCON-1072: Disabled programming of FSJoin Relays with Common Single 75 pattern.
•	PSSCON-1071: Relay Wiring Reports now opens and generates as it should.
•	PSSCON-1051: New 21 Button Keypad.
•	PSSCON-1050: New 17 Button W/Rotary keypad.
Build 3.6.0.0
Release Notes:
•	PSSCON-733: New GUI application for FSDirect.
•	PSSCON-1068: Enhanced Search filter for Tone Selection.
•	PSSCON-1067: Miscellaneous Tab Backlighting + - Value Adjusted.
•	PSSCON-1066: New supported Vehicles: 2024 Models Chevy: Colorado 1500, Silverado 1500, Tahoe PPV. Ford: Escape, Explorer, F250, F450, F550, F650, Mustang Mach Escape, Ranger. Freightliner: M2 106, M2 112. Hino: L6. International: HX, MV. Kenworth: T280, T380, T480, T880. Mitsubishi: Outlander. Ram: 4500, 5500. 2025 Models Chevy: Blazer EV PPV, Tahoe. Freightliner: M2 106, M2 112. International: HX, MV. Jeep: Grand Cherokee. Kenworth: T280, T380, T480, T880
•	PSSCON-1065: Introduced a new Auxiliary Device Page.
•	PSSCON-1064: Added a New Lightbar Device Page.
•	PSSCON-1063: Remodeled Splash Screen Page for an improved user experience.
•	PSSCON-1039: Implemented a new “Sweep T13” lightbar pattern.
•	PSSCON-1024: Added a new voice message: “Step Away from Vehicle.”
•	PSSCON-1062: Fixed an issue where Perimeter Breach Warning System inputs were not refreshing on load.
•	PSSCON-1048: Resolved issue where 21” Allegiant was not populating bed light on Detect LED.
•	PSSCON-1045: Renamed and reordered Recover Mode to prevent confusion.
•	PSSCON-1044: New FSJoin Devices Firmware Images to Version (1.3.0.0).
•	PSSCON-1043: New Keypad Firmware Image to Version (3.1.0.6).
•	PSSCON-1036: Removed BATT Input from the Controller Type Serial Interface Module.
•	PSSCON-1025: Fixed an issue where Tristate refresh resets when switching user modes.
•	PSSCON-1021: Enabled PW100 and PA300 support for PBW.
•	PSSCON-1020: Fixed Expansion Module BCM + Off button bug.
•	PSSCON-1018: Firmware Updates: Pathway Version (1.1.0.7) Pathfinder Version (3.2.0.12) SIM Version (1.2.0.6) 
•	PSSCON-1014: Fixed Pursuit Pattern in all lightbars to include white in pattern preview.
•	PSSCON-1013: Resolved unhandled null phase in FSJoin Relays, which was causing programming errors.
•	PSSCON-1011: Fixed incorrect commands loaded for Signal Master fast and low power.
•	PSSCON-1004: Renamed devices to align with Marketing specifications.
•	PSSCON-979: Ensured BCM Connect/Disconnect responds correctly when all modules are highlighted.
Build 3.5.0.1
Release Notes:
•	PSSCON-1003: Resolved a visual issue in the Configuration Viewer where "Tone Off" was not correctly displayed for Channel 1 and Channel 2.
•	PSSCON-1002: Fixed FSJoin Relay Tab BCM Disconnect Label (visual Bug)
•	PSSCON-1001: Fixed BCM Disconnect/Connect status did not consistently update visually on relays when toggled.
•	PSSCON-998: Validation implemented to prevent adding the Perimeter Breach Warning System without a supported amplifier.
•	PSSCON-998: Validation implemented to prevent adding the Perimeter Breach Warning System without a supported amplifier.
•	PSSCON-997: New Pathway Firmware Version(1.1.0.6).
•	PSSCON-996: New PF400/PF400Q Firmware Version(1.0.0.19).
•	PSSCON-995: New Pathfinder Firmware Version(3.2.0.12).
•	PSSCON-994: Support added for the 51 “VALR/INTG Passenger Board (board number 20000639).
•	PSSCON-988: visual bug fix related to with Bedlight feature.
Build 3.5.0.0
Release Notes:
•	PSSCON-974: New PF400/PF400Q Firmware Version(1.0.0.18).
•	PSSCON-961: New Pathfinder Firmware Version(3.2.0.9).
•	PSSCON-959: Updated images in the 32 Channel Relay Wiring Report Diagram for better clarity.
•	PSSCON-958: Adjusted the Low Power Mode activation checkbox in PTEK files for enhanced usability.
•	PSSCON-957: Added scroll wheel support in the Configuration Viewer layout within PTEK files.
•	PSSCON-956: New Audible Alarm Feature added.
•	PSSCON-954: PSSCON-954: Added a new voice message: "Step Away from the Vehicle".
•	PSSCON-616: New Reliant S2 Lightbar.
•	PSSCON-778: New Perimeter Breach Warning System.

Build 3.4.0.24
Release Notes:
•	PSSCON-953: Default Can Values Updated for 2024 Mitsubishi Outlander.
•	PSSCON-952: Default Can Values Updated for 2025 Police Interceptor.
•	PSSCON-951: Default Can Values Updated for 2024 Ford F150.
•	PSSCON-950: Default Can Values Updated for 2024 Honda Odyssey.
•	PSSCON-949: Default Can Values Updated for 2024 Ram 1500.
•	PSSCON-948: Default Can Values Updated for 2024 Chevy Blazer.
•	PSSCON-947: Default Can Values Updated for 2023 Ford F250.
•	PSSCON-946: Default Can Values Updated for 2023 Chevy Sierra 1500.
•	PSSCON-945: Default Can Values Updated for 2023 Chevy Silverado 1500.
•	PSSCON-944: Default Can Values Updated for 2024 Ford Mustang.
•	PSSCON-943: Default Can Values Updated for 2023 Ford F150.
•	PSSCON-942: Default Can Values Updated for 2021 Chevy Tahoe.
•	PSSCON-941: Resolved an issue with BCM Features getting cleared from configuration files when loaded into the GUI for Expansion Modules.
•	PSSCON-940: CAN support added for 2024 Mitsubishi Outlander.
•	PSSCON-935: Resolved an issue with Layer Cruise Functionality for 24/32 Channel Expansion Modules.
Build 3.4.0.22
Release Notes:
•	PSSCON-935: Resolved an issue with Layer Cruise Functionality for 24/32 Channel Expansion Modules.
Build 3.4.0.21
Release Notes:
•	PSSCON-925: CAN support added for 2024 Ford F150.
•	PSSCON-924: CAN support added for 2025 Ford Police Interceptor Utility.
•	PSSCON-923: New Firmware for PW100 Version(1.0.0.5).
•	PSSCON-901: Minimize Screen on startup fixed.
•	PSSCON-899: Q Tones no longer get erased when flasher is full.
•	PSSCON-896: FSJoin BCM Feature is now Correctly loaded in the process table.
•	PSSCON-893: Custom Relay Wiring report size adjustment.
•	PSSCON-891: New Firmware for PF400/PF400Q Version (1.0.0.14).
•	PSSCON-890: New Firmware for Keypad Version (3.0.0.16).
•	PSSCON-887: Fixed Gui crashing when clicking tone preview without a tone selection.
•	PSSCON-885: Fixed the issue where original message binding is lost when changing language settings for voice messages.
•	PSSCON-884: Improved PF400/PF400Q configuration inspection, particularly on Channels 3 and 4, ensuring the correct 'MID' settings are applied. 
•	PSSCON-883: Fixed the issue where voice messages assignment to Channels 3 and 4 triggers a restart of the amplifier.
•	PSSCON-882: Update Lightbar pattern definitions.
•	PSSCON-879: Fixed the issue with 'BCM Disconnect' being out of sync.
•	PSSCON-876: Default key position for 2023 Ford F150, 2023 F250, and 2024 Ford Mustang updated.
•	PSSCON-875: Updated the bus speed for Chevy Blazer 2024.
•	PSSCON-874: Fixed the issue where 'BCM Disconnect' became unchecked while configuring a relay in FSjoin Relays Tab.
•	PSSCON-873: Fixed the issue where intensity output controller did not apply to steady burn output controller.
•	PSSCON-870: Fixed the issue where flasher phase reset to 0 when dim intensity is updated for a fSjoin relay.
•	PSSCON-869: Removed 'Application Version is Null' from log extracts.
•	PSSCON-867: Fixed a display issue in FSjoin Relays tab after importing new relay configurations.
•	PSSCON-865: Fixed the issue where relay wiring report names were not updating after changes on the hardware page.
•	PSSCON-860: Added Pathway instructions Manual.
•	PSSCON-859: Blocked firmware updates for the 24 Channel Module, CNSM and ILS, if they report firmware version 1.1.0.64.
•	PSSCON-857: Added Pathway to the bootloader firmware recovery choices in the GUI.
•	PSSCON-853: Fixed the issue with the software minimizing behavior.
•	PSSCON-846: Fixed bug in Configuration Viewer when searching for all capitalized relay names.
•	PSSCON-845: Fixed the issue where relay name changes in diagnostics for the 24 Channel and 32 channel expansion modules were not saved.
Build 3.4.0.15
Release Notes:
•	PSSCON-891: New Firmware for PF400/PF400Q Version (1.0.0.14).
•	PSSCON-890: New Firmware for Keypad Version (3.0.0.16).
•	PSSCON-887: Fixed Gui crashing when clicking tone preview without a tone selection.
•	PSSCON-885: Fixed the issue where original message binding is lost when changing language settings for voice messages.
•	PSSCON-884: Improved PF400/PF400Q configuration inspection, particularly on Channels 3 and 4, ensuring the correct 'MID' settings are applied. 
•	PSSCON-883: Fixed the issue where voice messages assignment to Channels 3 and 4 triggers a restart of the amplifier.
•	PSSCON-882: Update Lightbar pattern definitions.
•	PSSCON-879: Fixed the issue with 'BCM Disconnect' being out of sync.
•	PSSCON-876: Default key position for 2023 Ford F150, 2023 F250, and 2024 Ford Mustang updated.
•	PSSCON-875: Updated the bus speed for Chevy Blazer 2024.
•	PSSCON-874: Fixed the issue where 'BCM Disconnect' became unchecked while configuring a relay in FSjoin Relays Tab.
•	PSSCON-873: Fixed the issue where intensity output controller did not apply to steady burn output controller.
•	PSSCON-870: Fixed the issue where flasher phase reset to 0 when dim intensity is updated for a fsjoin relay.
•	PSSCON-869: Removed 'Application Version is Null' from log extracts.
•	PSSCON-867: Fixed a display issue in FSJoin Relays tab after importing new relay configurations.
•	PSSCON-865: Fixed the issue where relay wiring report names were not updating after changes on the hardware page.
•	PSSCON-860: Added Pathway instructions Manual.
•	PSSCON-859: Blocked firmware updates for the 24 Channel Module, CNSM and ILS, if they report firmware version 1.1.0.64.
•	PSSCON-857: Added Pathway to the bootloader firmware recovery choices in the GUI.
•	PSSCON-853: Fixed the issue with the software minimizing behavior.
•	PSSCON-846: Fixed bug in Configuration Viewer when searching for all capitalized relay names.
•	PSSCON-845: Fixed the issue where relay name changes in diagnostics for the 24 Channel and 32 channel expansion modules were not saved.

Build 3.4.0.0
Release Notes:
•	PSSCON-843: Can Support for 2024 Ram 1500.
•	PSSCON-826: Improved PW100 Relays disconnection and reconnection functionality.
•	PSSCON-822: Introducing new firmware (version 1.2.0.8) for all FSJoin devices, ensuring optimal performance and stability.
•	PSSCON-821: Added support for Blank Default Configurations across all Amplifiers, providing more flexibility in customization.
•	PSSCON-819: Addressed Simple Flash Pattern inconsistency - 99FPM now corrected to 95FPM, ensuring accurate and consistent flash patterns.
•	PSSCON-818: Enabled steering wheel Angle can message support for 2021 Durango Pursuit, enhancing compatibility and integration.
•	PSSCON-817: Enhanced display names on Amplifier Hardware Page, improving readability and user experience.
•	PSSCON-816: Updated 2CH Flasher Pattern Name from "SC DOT 81" to "Reverse Double Pulse", aligning with industry standards.
•	PSSCON-815: Modified Tone Unitrol Wail Coast settings to "Unitrol wail with Coast OFF", allowing for more precise control of audio outputs.
•	PSSCON-814: PW100 Seventeen Button now supports a Default configuration, simplifying setup and configuration.
•	PSSCON-810: Enhanced ALGT 21IN Auto Detection to Include Bed Light Support and Prevent Customer Confusion, ensuring accurate detection and preventing user confusion.
•	PSSCON-807: Added Support for Standalone Amplifiers Default configurations, providing more options for standalone amplifier setups.
•	PSSCON-806: Allegiant Lightbars now Supports Red/White/bed light option, giving users more flexibility in lightbar configurations.
•	PSSCON-805: Allowed Tone Off setting to be independently applied to Button Status ON and OFF, offering greater customization for audio outputs.
•	PSSCON-801: Included 2023 Ford F250 in the GUI for easy selection, making vehicle selection more convenient.
•	PSSCON-788: Enabled auto-detection for 21-inch ALG LED, simplifying setup and configuration.
•	PSSCON-772: Updated Can Channel for Ford F150 2023, ensuring compatibility with the latest vehicle models.
•	PSSCON-739: Added support for EQ2B Keypad rotary switch backlighting, enhancing visibility and usability.
•	PSSCON-759: Refactored default configurations for better organization and usability, making it easier to find and use default settings.
•	PSSCON-713: Added FSJoin Relays Tab for easier management of relay modules, streamlining relay configuration and control.
•	PSSCON-764: Included FS Fade feature options now supported for FSJoin Relays/Cutoffs Tab/Steady Burn Tab/Simple Patterns Tab.
•	PSSCON-803: Fixed the bug that prevented Relay Wiring Report and Diagnostics for FSjoin Relay Modules, ensuring accurate diagnostics and reporting.
•	PSSCON-798: Corrected the spelling error in the import tone pop-up message, improving overall user experience.
•	PSSCON-783: Ensured that Tone off setting is saved properly for off Button, maintaining user preferences and settings.
•	PSSCON-773: Resolved the issue with GUI crashing caused by Keypad Led Miscellaneous Tab, improving stability and usability.
•	PSSCON-785: Removed low Amp-rated relays from Diagnostics, providing more accurate diagnostics results.
•	PSSCON-779: Included 2024 Chevy Blazer in the GUI for easy selection, expanding vehicle compatibility options.
•	PSSCON-752: Added support for PF400Q devices, increasing compatibility and integration options.
•	PSSCON-605: Added support for PF400 devices, offering more flexibility in device selection.
•	PSSCON-736: Included support for new speaker selection, allowing for a wider range of speaker options.
•	PSSCON-681: Included 32 Channel Expansion Module in the GUI with a detailed wiring report for 32 Channel Relays.

Build 3.3.0.0
Release Notes:
•	PSSCON 618 - Ground Activated IGN removed from GUI.
•	PSSCON 638 - New 21 “Allegiant lightbar.
•	PSSCON 678 - Disallow dimming when cruise is selected in (FSjoin Legacy Mode).
•	PSSCON 685 - Reconfigured splash screen.
•	PSSCON 692 - Implement default configuration file clear/overwrite.
•	PSSCON 706 - Add a filter/search option for flash patterns and vehicles.
•	PSSCON 708 - Resolved Pathfinder relay intensity bug.
•	PSSCON 709 - PA300 Amp no longer Supports all keypads.
•	PSSCON 710 - 24 Channel Expansion Module now displays the correct intensity percentage in the configuration viewer.
•	PSSCON 711 - Screen now maximizes on launch.
•	PSSCON 712 - Relay wiring report now includes additional columns for upfit wire color and product wire color.
•	PSSCON 714 - Fixed Dodge Durango secure park Can message issue. 
•	PSSCON 715 - Updated default configuration for PW100 and PA300.
•	PSSCON 717 - Users can now edit the customer defined relay report fields and print within the GUI.
•	PSSCON 722 - Improved visibility of relays in both Light and Dark mode for better user interaction. 
•	PSSCON 724 - Firmware update for Pathfinder (3.1.0.17), Pathway (1.0.0.2), Keypad (3.0.0.15), Sim (1.1.0.14).
•	PSSCON 732 - Auto advancing step synchronization now supported when Double Press to stop steps and Auto-advance steps is enabled.
•	PSSCON 737 - Add Vehicle CAN Support for the Latest Models: the 2020 Toyota Tundra, 2022 Ford Maverick, 2022 Tesla Model 3, 2023 Chevy Silverado, 2023 Ford F150, 2023 GMC Sierra, and 2024 Ford Mustang.
•	PSSCON 740 - Enhanced Visibility: The taskbar is now visible when the screen is maximized, providing a better user experience. Improved Window Behavior: In maximized mode, the application will no longer stay on top of other windows, ensuring a seamless Fullscreen experience.
•	PSSCON 741 - BarcodeProcessLoader now includes support for ALGT21.

Build 3.2.0.0
Release Notes:
•	PSSCON 599 - Addition of new PA300 Keypad and PA300 amplifier.
•	PSSCON 604 - Introduction of new Pathway 100 amplifier.
•	PSSCON 674 - Inclusion of the option to enable/disable low power mode for locked files with low tones.
•	PSSCON 687 - Fix for application crashes that occurred when selecting Handheld default configuration.
•	PSSCON 688 - Fix for application crashes that occurred when battery voltage was set to 0.
•	PSSCON 691 - Correction of PF200 Default Configuration.
•	PSSCON 693 - Increase of Battery Input support to up to 16 Volts.
•	PSSCON 694 - Fix of Legacy Lightbar Pattern Dropdown List UI bug and removal of support for flash patterns 27 or 28.
•	PSSCON 695 - Fix for Relay Dim Checkbox that previously caused crashes.
•	PSSCON 696 - Correction of PF100 Relays Supported Display.
•	PSSCON 697 - Fix for 17 Button Default PCF.
•	PSSCON 700 - Introduction of new Sim firmware (version 1.1.0.13).
•	PSSCON 703 - Elimination of duplicate outputs in Configuration Viewer from Local PA and PA.
•	PSSCON 704 - Fix for Reliant Board Mapping.
•	PSSCON 707 – Allow User to select a front Fsjoin with a Rear CN Signal master.
Build 3.1.0.33
Release Notes:
•	PSSCON 624 - New PA4000 Keypad/Model Released.
•	PSSCON 664 - Single 113/116 flash Rates fixed
•	PSSCON 663 - Front SM option added to Fsjoin Products.
•	PSSCON 661 - 24 channel Relay Intensity bug fixed “no longer resets to 0”
•	PSSCON 658 - Ignition feature not saving shut down option.
•	PSSCON 657 - Release notes no longer can be Modified.
•	PSSCON 655 - Selecting OFF command in On Step issue.
•	PSSCON 649 - Support SIM Feature state Diagnostics.
•	PSSCON 617 - Allegiant Now supports Amber/White/Bedlight option.
•	PSSCON 669 - Firmware Update for Pathfinder Amplifier and Keypad.
•	PSSCON 667 - Chevy Tahoe 2021 Transmission Signals Fixed.
•	PSSCON 623 - Unify Hardware Selection screens.
•	PSSCON 619 - removed Autodetect Led from front and rear FSJoin CN.
•	PSSCON 679 – Firmware Update For PF Amp(3.1.0.14), Keypad(3.0.0.13) , SIM(1.1.0.12), PWY Amp(1.0.0.0).
•	PSSCON 677 -when adding an Fsjoin Rear and Front Cn, the Legacy products are no longer Selectable, Also on first UI interface if FsJoin front rear CN is selected and user selects Legacy Front or Rear it will uncheck Fsjoin and vise versa.
•	PSSCON 676 - Add OBD/CAN capabilities for PA4000
•	PSSCON 675 - Remove EQ2B & Remote Keypad From Standalone Lightbar Controller.
•	PSSCON 673 - Sync Module Duplicates can no longer be added on Hardware Page.
•	PSSCON 672 - Relay Wiring Report and Current Limit Fixed no longer crashes or fails to open.
•	PSSCON 671 - The ignition Check Box Visibility is only visible for stand alone controllers 4,6,9 controllers.
•	PSSCON 670 - Default Button Colors On/Off no longer overlapping each other.
Build 3.1.0.31
Release Notes:
•	PSSCON 653 - BedLight not saving for FSJoin Allegiant.
•	PSSCON 648 - Application crashing when opening 2021 Tahoe PFC file. 
•	PSSCON 644 - Update Pathfinder Installation and Maintenance manuals to latest revision.
•	PSSCON 643 - Update SIM firmware Image for next release which includes 24-Channel module support.
Build 3.1.0.30
Release Notes:
•	Firmware update for 24 Channel Expansion Module from a bad version in Build 3.1.0.29
Build 3.1.0.29
Release Notes:
•	Update Rumbler Tone files
•	Resolved an issue related to flashing FS-Join lightbar configuration.
•	Firmware update in amplifier/ stand alone lightbar controller/serial interface module to fix configuration corruption during unexpected power loss when configured with FSJoin or a 24 Channel Expansion Module
•	Firmware update in FSJoin products to fix Progressive pattern
•	Firmware update in amplifier to fix relay dimming issue
•	2022 Chevy Silverado 1500 CAN signals added
•	2022 Ford E-Transit signals added
•	2021 Ford Mustang Mach E signals added
•	2021 Dodge RAM 1500 signals added
•	2021 Ford Transit signals added
•	2021 Dodge Durango (Pursuit) signals added
•	2020 Ford Police Interceptor Utility signal update
Build 3.1.0.17
Release Notes:
•	New voice messages added: Tank levels + “Officer needs help”
•	On Scene Sync Module added
•	CAN simulator added
Build 3.1.0.16
Release Notes:
•	CAN signals added for 2021 Chevy Tahoe
Build 3.1.0.15
Release Notes:
•	Audio synchronization added
Build 3.1.0.13
Release Notes:
•	Firmware updated in amplifier and keypad to fix various commands not turning off
Build 3.1.0.12
Release Notes:
•	FSJoin CNSM added
•	Updated training guide
Build 3.1.0.9
•	2021 F250 CAN signals added
•	“Progressive” pattern added to all FSJoin devices
Build 3.1.0.5
Release Notes:
•	2021 Dodge Durango/Durango Pursuit CAN signals added
•	2020 Jeep Wrangler CAN signals added
Build 3.1.0.2
Release Notes:
•	2021 Ford Expedition CAN signals added
Build 3.1.0.1
Release Notes:
•	2019 Chevy Express CAN signals added
Build 2.3.1.11
Release Notes:
•	Feature state diagnostics added
Build 2.3.1.10
Release Notes:
•	Low power amplifier mode added
•	Speaker diagnostics added
•	2020 PIU backup sensor signals added
Build 2.3.1.8
Release Notes:
•	Relay programming UI updated
Build 2.3.1.6
Release Notes:
•	CAN Diagnostics added
•	FSJoin released
•	8 more virtual inputs added
Build 2.3.1.3
Release Notes:
•	Wipers, Cruise signals added to 2019/2020 FPIU
Build 2.3.1.0
Release Notes:
•	17-button controller added
Build 2.3.0.10
Release Notes:
•	OBD-II data added for 2020 Traverse, high beam latched/momentary added to 2020 FPIU
•	Amplifier firmware updated to 3.0.0.8
Build 2.3.0.7
Release Notes:
•	Amplifier firmware updated to 3.0.0.7
Build 2.3.0.6
Release Notes:
•	OBD-II support added for 2020 Escape/F250/GMC Sierra
Build 2.3.0.5
Release Notes:
•	Amplifier firmware version 3.0.0.6 released
o	Includes fixes for timed shutdown and control head blinking
Build 2.3.0.3
Release Notes:
•	24 Channel Expansion Module added
•	Amplifier firmware updated
•	Expansion module firmware updated
•	Keypad firmware updated
•	Power distribution module firmware updated
•	Wake-on-CAN added
•	Purple/Amber buttons added to Handheld, 4/6/9 Button keypads
•	Multiple blinking styles added for all buttons
•	Technician files added
•	Low PA/Radio gain bugfix
Build 2.2.0.6
Release Notes:
•	New Curfew + K9 voice messages
•	2018/2019 Interceptor Utility transmission range signal fixed in low gears
•	Added 2020 Dodge Charger, Chevy Tahoe, and Ford F150
•	CAN signal names standardized
•	Bugfix for being unable to delete some ILS patterns
•	Added ability to generate a PDF based on configuration viewer searches
Build 2.2.0.5
Release Notes:
•	Dark mode fixed for 2-channel flasher
•	Keypad SM Warn command added to 17-button default
•	2020 Interceptor Utility transmission range signal fixed in low gears
•	File extension changed from .json to .pfc (files remain backwards compatible)
Build 2.2.0.4
Release Notes:
•	Bugfix for failed file extraction
•	Bugfix for corrupted files with an external relay module
Build 2.2.0.3
Release Notes:
•	COVID-19 voice messages
•	Fix for Rear ILS SM Fast deselecting itself
•	Fix for scenario where missing polarity settings could corrupt a .json file
•	Fix for Amplifier forgetting OBD settings
•	2 Channel Flasher Added
Build 2.2.0.2
Release Notes:
•	Releases firmware version 2.1.1.4
•	New 2020 Police Interceptor Utility signals added (Steering wheel angle, Brake pedal position, Ambient Light)
•	Bugfix where loading a file with a custom tone could crash
Build 2.2.0.1
Release Notes:
•	Modified 2020 Interceptor Utility CAN Signals
o	Steering wheel button 1 & 2 flipped; Brake signal improved; Key in/Key out signal added
•	Added log file extraction (help > extract log files)
•	Added the ability to open configuration notes on file load
•	Bugfix to remove remote activations after an input is deleted
•	Added PF100 to hardware selection page
•	Fixed bug where you would be asked to re-import a standard voice message
Build 2.2.0.0
Release Notes:
•	Amplifier firmware version 2.1.1.2
•	Keypad firmware version 2.0.0.2
o	Includes cold-weather fix
Build 2.1.0.0
Release Notes:
•	Keypad SignalMaster indicator now independently selectable
•	Keypad SignalMaster bugfix for default configuration
•	Shutdown wizard bugfix
•	Vehicle name now shows over CAN inputs
•	Bugfix for Expansion Module relays 13/14/15 Intensity Settings
Build 2.0.0.31
Release Notes:
•	Diagnostics added
Build 2.0.0.30
Release Notes:
•	Fix for tone preview always previewing step 1
•	Added 2019 Challenger/Mustang/Acadia/Equinox/Expedition/Ranger
•	Firmware version 2.1.1.1
Build 2.0.0.29
Release Notes:
•	Configuration reads password-protected
•	Configuration reads remember user-given configuration name
•	Power Distribution Module tab moved closer to Pathfinder/ExpansionModule relays
•	Allow multiple instances of the application to be open at once
•	Current Limits added to the Power Distribution Module
•	Various USB communication bugfixes
•	Fix for unneeded tone-file flashing
•	Remote activation tab updated to display context-relevant names
Build 2.0.0.27
Release Notes:
•	Power Distribution Module added
•	Amplifier firmware version 2.1.1.0 released
•	Expansion module firmware version 2.0.0.2 released
•	Keypad firmware version 2.0.0.0 released
•	Hardware page UI tweaks
•	Bugfix where old files with a secondary expansion module may crash
•	Softer English voice messages added
•	Padding added to voice messages
Build 2.0.0.26
Release Notes:
•	Bugfix for various names being displayed incorrectly
•	Scrollbar added to custom commands page
•	Configuration notes section added
•	Bugfix for “phantom” CAN signals selected but not enabled
•	Protections added to the firmware update procedure
•	CAN data added for 2019 Tahoe, Grand Cherokee, and Suburban
•	CAN data modified for 2020 Ford Police Interceptor Utility
•	Bugfix for missing tones
•	Amplifier firmware version reverted to 2.1.0.13
Build 2.0.0.25
Release Notes:
•	Bugfix for files flashing more often than necessary
•	Firmware update UI cleaned up
•	Added ability to lock a device’s configuration
•	Added multi-language voice messages
•	Updated 17-button default configuration
•	Added information to configuration report
Build 2.0.0.24
Release Notes:
•	Added notification for updates to the software
•	Fixed a bug where files with an external relay module would crash on load
•	Added standard library of voice messages
•	Added a note displaying how much space is left on the Pathfinder
•	PA is now configured by default
•	Bug fixed where turning a relay off would load an off command in the off step
•	Fixed scenario where PA could be mis-configured (PA shows ON but no audio comes through)
Build 2.0.0.23
Release Notes:
•	Clone button text color changed for increased visibility
•	Confirmation dialog added when changing the step count of a feature
•	Lightbar page only shows features supported by that model
•	Bugfix for being able to occasionally select 7 dependencies
•	Bugfix for buttons 13 and 14 being swapped on the handheld
•	Bugfix for no backlighting on handheld/smart controller
Build 2.0.0.22
Release Notes:
•	Tone wizard will no longer clobber slide switch patterns and relays (still eliminates tones, remote activations)
•	UI improvements on priorities page
•	“Open priorities” and “open grouping” buttons added to properties tab
•	QOL updates for configuration report (CAN/Inputs/VRTLs renamed)
•	Most windows are now draggable
•	Bugfix for CAN signals from a previously opened configuration appearing in a new file
•	Added ability to lock the gain for PA/Radio (primarily for the Smart Controller)
•	Releases firmware version 2.1.0.13
Build 2.0.0.21
Release Notes:
•	Application automatically will enter the main view when an existing JSON file is loaded
•	Minimal configs (Blank config with rumbler setup etc) no longer appear if an unsupported keypad is selected
•	Improved backlighting slider tooltips
•	Toggle/step option added for general purpose inputs in standard mode (previously only available in advanced)
•	Relay intensity sliders added in standard mode (previously only available in advanced)
•	Bugfix for ILS tab having neither front or rear ILS selected
•	“Select your vehicle” removed from Vehicle tab
•	New features now start with the highest priority (previously lowest priority)
•	Bugfix for properties tab being open without a selected button
Build 2.0.0.20
Release Notes:
•	Changed text color for inputs with multiple features
•	Bugfix where SignalMaster sync wouldn’t work on the local keypad — Older files may still be affected
•	Bugfix for being unable to remove a SignalMaster sync command in an older file
•	Bugfix for application crash on tone preview
•	Duplicate parking brake signal in the 2020 Police Interceptor Utility removed
Build 2.0.0.19
Release Notes:
•	Release notes added to application
•	Fixed bug if “Open file” could not find the last used drive
•	Fixed bug where loading a .json file configured with an ILS would throw an error
Build 2.0.0.18
Release Notes:
•	Removed the ability to group same-input features
•	Relay wiring report for Pathfinder and Expansion Module consolidated
•	Signal master changed to SignalMaster in various locations
•	Path finder/PathFinder changed to Pathfinder in various locations
•	Updated Logo
•	Ability to preview custom tones added
•	CAN data for 2019 Impala/Silverado/F150 added
•	Checkboxes removed from the ILS tab
•	Checkboxes removed from the CN SignalMaster tab
•	UI enhancements for smaller screen sizes
•	Help-text added for horn-ring transfer
•	Filter added for dependencies column in configuration viewer
•	Volume input added to remote handheld
•	Release notes added to installer
•	Releases FRWVER 2.1.0.12
•	"Hardware" view added
•	Content is now dynamic based on the hardware you select, hiding information irrelevant to your system
Build 2.0.0.17
Release Notes:
• Support for file associations (double click file to open in application)
• New expansion module quick start guide, swapped J9 and J12 connectors
• Rename CHMSL and Sense line to CHMSL Cutoff and Sense Line Bypass
• Releases Pathfinder AMP FRWVER 2.1.0.11
• Switching between momentary/toggle no longer clears your configuration
• Bugfix for invisible remote activation command created by tone configuration wizard
• Bugfix for double shutdown command being set
• Bugfix for unplugging the device while flashing a custom tone
• Bugfix for SignalMaster fast/low incorrectly deselecting fast/low power off
• Bugfix for blank/default files: can't select 30 functions on volume button
• Bugfix for front lightbar command being displayed as signalmaster sync
Build 2.0.0.16
Release Notes:
• Releases FRWVER 2.1.0.10
• Fixes a bug where the application could fail to extract a configuration created in an older version
• Fixes a bug where there could be an "invisible" backlighting command on the volume button
• Installer size reduced (~100MB to ~20MB)
• Adds support for software fuses on pathfinder and expansion module relays
• Releases expansion module firmware version 2.0.0.1
• Checkbox added to SirenFunctions tab to help with syncing tones across channels.